For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Disconnect the fuel tank pressure sensor electrical connector (1).

Important: There are alignment features on the canister, however, there are no locking tabs on the sensor/canister. The sensor is held into the canister by the tight fit of the multi-lip seal.

3. Remove the fuel tank pressure sensor from the evaporative emission (EVAP) canister.

### Installation Procedure

Important: There are alignment features on the canister, however, there are no locking tabs on the sensor/canister. The sensor is held into the canister by the tight fit of the multi-lip seal.

1. Install the fuel tank pressure sensor to the EVAP canister until fully seated.
2. Connect the fuel tank pressure sensor electrical connector (1).
3. Lower the vehicle.