For 1990-2009 cars

1. Install the skid plate.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the skid plate bolts.

Tighten
Tighten the skid plate bolts to 10 N·m (89 lb in).

3. Install the oil pan drain plug and NEW O-ring seal.

Tighten
Tighten the oil pan drain plug to 25 N·m(18 lb ft).

4. Install the NEW oil suction pipe O-ring.
5. Install the oil suction pipe.
6. Install the oil suction pipe bolts.

Tighten
Tighten the oil suction pipe bolt to 10 N·m (89 lb in).

7. Install the oil pan scraper.
8. Install the oil pan scraper bolts.

Tighten
Tighten the oil pan scraper bolts to 10 N·m (89 lb in).