For 1990-2009 cars

#### Special Tools

J 28410 Gasket Remover

### Cleaning Procedure

1. Remove any old thread sealant, gasket material or sealant using J 28410 .
2. Clean the oil pan and oil pan components in solvent.
3. Clean out debris from the bolt holes.

Caution: Refer to Safety Glasses Caution in the Preface section.

4. Dry the oil pan and oil pan components with compressed air.

### Inspection Procedure

1. Inspect the exterior of the oil pan for the following conditions:

• | Dents or damage to the exterior (1)

• | Damage to the drain plug or drain plug hole (2)

• | Damage to the transaxle brace mounting bosses (3)

• | Damage to the transaxle mounting bosses (4)

2. Inspect the interior of the oil pan for the following conditions:

• | Gouges or damage to the oil pan sealing surfaces (1)

• | Damage to the oil pan scraper mounting holes (2)

• | Damage to the bolt holes (3)

3. Repair or replace the oil pan and/or oil pan components as necessary.