For 1990-2009 cars

Callout | Component Name
--- | ---
Tail Lamp Assembly Replacement Preliminary Procedure

1. Open the rear compartment lid.
2. Remove the rear compartment side trim panel assembly. Refer to Side Trim Panel Replacement ñ Rear Compartment in Body Rear End.

1 | Tail Lamp Nuts (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (53 lb in)
2 | Tail Lamp Electrical Connector
3 | Tail Lamp Assembly Tip The tail lamp assembly is LED and there are no replaceable bulbs. The lamp assembly must be replaced as an assembly.