For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation .

Important: Hold the shaft link stud with a hex tool to prevent damage to the link seal.

3. Remove the stabilizer shaft link retaining nuts.
4. Remove the stabilizer shaft link from the stabilizer shaft.
5. Remove the stabilizer shaft link from the lower control arm.

### Installation Procedure

1. Install the stabilizer shaft link to the lower control arm.
2. Install the stabilizer shaft link to the stabilizer shaft.

Notice: Refer to Fastener Notice in the Preface section.

Important: Hold the shaft link stud with a hex tool to prevent damage to the link seal.

3. Install the stabilizer shaft link retaining nuts.

Tighten
Tighten the nuts to 66 N·m (49 lb ft).

4. Install the tire and wheel. Refer to Tire and Wheel Removal and Installation .
5. Lower the vehicle.