For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation.
3. Remove the brake rotor. Refer to Front Brake Rotor Replacement.
4. Disconnect the antilock brake system (ABS) electrical connector.
5. Remove the electrical connector from the splash shield.
6. Remove the wheel bearing/hub mounting bolts.
7. Remove the wheel bearing/hub.

### Installation Procedure

1. Install the wheel bearing/hub.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the wheel bearing/hub mounting bolts.

Tighten
Tighten the bolts to 135 N·m (100 lb ft).

3. Install the electrical connector to the splash shield.
4. Connect the ABS electrical connector.
5. Install the brake rotor. Refer to Front Brake Rotor Replacement.
6. Install the tire and wheel. Refer to Tire and Wheel Removal and Installation.
7. Lower the vehicle.