For 1990-2009 cars

### Removal Procedure

1. Remove the screws securing the insulator.
2. Disconnect the electrical connector and remove the insulator.

### Installation Procedure

1. Connect the electrical connector and install the insulator.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the screws securing the insulator.

Tighten
Tighten the screws to 2 N·m (18 lb in).