For 1990-2009 cars

#### Special Tools

J 39946 Crankshaft Socket - 4.0L and 4.6L

1. Ensure the crankshaft is in the top dead center (TDC) position for the number one cylinder using the J 39946 .

Notice: Refer to Valve Lifter Priming Notice in the Preface section.

2. Fill the stationary hydraulic lash adjuster (SHLA) with clean engine oil GM P/N 12378006 or equivalent. Take precautions to prevent scratching the pivot sphere area (1) of the SHLA.
3. Lubricate the SHLA bores of the cylinder head with clean engine oil GM P/N 12378006 or equivalent.
4. Install the SHLAs.
5. Apply a liberal amount of lubricant GM P/N 12345001 or equivalent to the SHLA sphere.