For 1990-2009 cars

Table 1: | Driver Door Module (DDM)
Table 2: | Instrument Panel Cluster (IPC)
Table 3: | Headlamp Control Module
Table 4: | Left Rear Door Module (LRDM)
Table 5: | Passenger Door Module (PDM)
Table 6: | Rear Integration Module (RIM)
Table 7: | Right Rear Door Module (RRDM)

#### Driver Door Module (DDM)

Scan Tool Output Control | Additional Menu Selections | Description
--- | --- | ---
Door Switch Backlight | Special Functions | The driver door module (DDM) illuminates the door switch incandescent lamps for 5 seconds when you select ON.
Exterior Courtesy Lamp | Special Functions | The DDM illuminates the exterior courtesy lamp for 5 seconds when you select ON and then fades to Off.
Lock Switch Indicator | Special Functions | The DDM illuminates the lock switch indicator LED for 5 seconds when you select ON.

#### Instrument Panel Cluster (IPC)

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
Display Test | Special Functions - IPC | The instrument panel cluster (IPC) activates the Display Test for 5 seconds when you select ON. The indicators should illuminate for 5 seconds.

#### Headlamp Control Module

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
Headlamp Motor Test | Special Functions | The headlamp leveling module moves the headlamp leveling motors up for 5 seconds when you select UP, then centers the motors. The headlamp leveling module moves the headlamp leveling motors down for 5 seconds when you select DOWN, then centers the motors.

#### Left Rear Door Module (LRDM)

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
Door Switch Backlight | Special Functions | The left rear door module (LRDM) illuminates the door switch incandescent lamps for 5 seconds when you select ON.

#### Passenger Door Module (PDM)

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
Door Switch Backlight | Special Functions | The passenger door module (PDM) illuminates the door switch incandescent lamps for 5 seconds when you select ON.
Exterior Courtesy Lamp | Special Functions | The PDM illuminates the exterior courtesy lamp for 5 seconds when you select ON and then fades to Off.
Lock Switch Indicator | Special Functions | The PDM illuminates the lock switch indicator LED for 5 seconds when you select ON.

#### Rear Integration Module (RIM)

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
Backup Lamp Relay | Special Functions - Output Control - Lighting | The rear integration module (RIM) activates the backup lamp relay for 5 seconds when you select ON. The backup lamps should illuminate for 5 seconds.
Courtesy Lamp w/Dimming | Special Functions - Output Control - Lighting | The RIM activates the courtesy lamps for 15 seconds when you select ON. The courtesy lamps will turn off through the theater dimming feature if you select OFF before the 15 second period has elapsed.
Courtesy Lamp w/o Dimming | Special Functions - Output Control - Lighting | The RIM activates the courtesy lamps for 5 seconds when you select ON. The courtesy lamps will turn off immediately if you select OFF before the 5 second period has elapsed.
Inadvertent Power Relay | Special Functions - Output Control - Lighting | The RIM deactivates the inadvertent power for 5 seconds when you select OFF. The interior lamps should be inoperative for 5 seconds.
LF Turn/Hazard Lamp | Special Functions - Output Control - Lighting | The RIM activates the left front turn/hazard lamps for 5 seconds when you select ON. The left front turn/hazard lamps should illuminate for 5 seconds.
LR Turn/Hazard Lamp | Special Functions - Output Control - Lighting | The RIM activates the left rear turn/hazard lamps for 5 seconds when you select ON. The left rear turn/hazard lamps should illuminate for 5 seconds.
Rear Fog Lamps | Special Functions - Output Control - Lighting | The RIM activates the rear fog lamp relay for 5 seconds when you select ON. The rear fog lamps should illuminate for 5 seconds.
RF Turn/Hazard Lamp | Special Functions - Output Control - Lighting | The RIM activates the right front turn/hazard lamps for 5 seconds when you select ON. The right front turn/hazard lamps should illuminate for 5 seconds.
RR Turn/Hazard Lamp | Special Functions - Output Control - Lighting | The RIM activates the right rear turn/hazard lamps for 5 seconds when you select ON. The right rear turn/hazard lamps should illuminate for 5 seconds.
Standing Lamp Relay | Special Functions - Output Control - Lighting | The RIM activates the standing lamp relay for 5 seconds when you select ON. The standing lamps should illuminate for 5 seconds.

#### Right Rear Door Module (RRDM)

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
Door Switch Backlight | Special Functions | The left rear door module (LRDM) illuminates the door switch incandescent lamps for 5 seconds when you select ON.