For 1990-2009 cars

### Removal Procedure

1. Remove the center floor console end panel. Refer to Front Floor Console Replacement.
2. Remove the screws securing the speaker to the console end panel.
3. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the screws securing the speaker to the console end panel.

Tighten
Tighten the screws to 2 N·m (18 lb in).

3. Install the center floor console end panel. Refer to Front Floor Console Replacement.