For 1990-2009 cars

### Removal Procedure

1. Remove the left sound insulator panel. Refer to Instrument Panel Insulator Replacement - Left Side.
2. Disconnect the left air temperature actuator electrical connector from the actuator.
3. Remove the left air temperature actuator screws.
4. Remove the left air temperature actuator.

### Installation Procedure

1. Install the left air temperature actuator.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the left air temperature actuator screws.

Tighten
Tighten the screws to 1 N·m (9 lb in).

3. Connect the left air temperature actuator electrical connector to the actuator.
4. Install the left sound insulator panel. Refer to Instrument Panel Insulator Replacement - Left Side.