For 1990-2009 cars

### Removal Procedure

1. Open the engine hood.
2. Remove the bolts from the cross vehicle brace.
3. Remove the cross vehicle brace from the vehicle.

### Installation Procedure

1. Install the cross vehicle brace to the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts to cross vehicle brace.

Tighten
Tighten the cross vehicle brace bolts to 112 N·m (80 lb ft).

3. Cover the engine hood.