For 1990-2009 cars

Callout | Component Name
--- | ---
Headlamp Ballast Assembly Replacement

• | Never open the high intensity discharge system ballast or the arc tube assembly starter.

• | Never probe between the high intensity discharge system ballast output connector and the arc tube assembly.

Preliminary Procedure

1. Remove the front fascia assembly. Refer to Fascia, Extension, Reinforcement and Impact Bar Replacement - Front Bumper in Bumpers.
2. Remove the front fascia assembly. Refer to Fascia, Extension, Reinforcement and Impact Bar Replacement - Front Bumper in Bumpers .

C

1 | Ballast Access Cover Screws Notice: Refer to Fastener Notice in the Preface section. Tighten: 3 N.m (27 lb in)
2 | Ballast Access Cover
3 | Headlamp Ballast Assembly