For 1990-2009 cars

Warning: Striker alignment is crucial for proper operation of the door systems. Do not hit the striker with a hammer or force alignment in any other way. Failure to properly adjust striker will result in excessive door efforts or extensive damage to door system operation which could result in personal injury.

1. Loosen the 2 striker screws.
2. Pull the striker outboard to the end of the adjustment travel.
3. Tighten the 2 striker screws so that the striker can still be moved.
4. Hold the outside door handle out and gently push the door flush against the body in order to locate the striker.
5. Slowly open the door.

Caution: Refer to Fastener Caution in the Preface section.

6. Secure the striker assembly.

Tighten
Tighten the striker screws to 27.5 N·m (20 lb ft).

7. After adjusting the striker, touch up any exposed or unpainted surfaces with body color paint.