For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Front Bumper Fascia Trim Assembly Refer to Front Bumper Fascia Replacement.
2 | Headlamp Washer Nozzle Screws Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
3 | Headlamp Washer Hose Assembly
4 | Headlamp Washer Nozzle Assembly

#### Procedure

1. Squeeze the locking tabs on the headlamp washer nozzle assembly together to remove and replace from the fascia.
2. Pull the nozzle shaft out and lock in place with the washer nozzle locking tabs.
3. Use a small flat-bladed tool to release the trim cover from the nozzle.