For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Orientate the alignment tab inside the passage sleeve with the slot in the electrical connector of the control solenoid valve assembly. Push the sleeve straight into the case bore and connector. Do NOT rotate the sleeve at any time. Ensure the sleeve is fully seated into the case. When the sleeve is properly installed, the distance from the case surface to the end of the sleeve should be 14-16 mm. Even though the correct electrical connections may still be maintained, failure to ensure proper installation of the sleeve may result in a fluid leak around the sleeve lip seal and into the sleeve cavity.

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the transmission fluid pan. Refer to Automatic Transmission Fluid, Fluid Pan and/or Filter Replacement.
3. Disconnect the vehicle wire harness electrical connector from the transmission electrical Connector Sleeve. Refer to Automatic Transmission Inline 16-Way Connector Description.

1 | Electrical Connector Slide Lock Tip Pull down on the slide lock to remove the sleeve. Push up on the slide lock after sleeve installation.
2 | Electrical Connector Sleeve Tip

• | Use the DT 47715 Electrical Connector Passage Sleeve Remover/Installer and J 42183 Driver Handle to remove and install the electrical connector sleeve.

• | The distance (a) from the case surface to the end of the sleeve should be 14-16 mm.

3 | O-Ring Seal (Qty: 2) Tip Use a NEW O-ring seal.
4 | Lip Seal Tip Use a NEW lip seal.