For 1990-2009 cars

Callout | Component Name
--- | ---

#### High Mounted Stop Lamp Emblem Assembly Replacement

1 | High Mounted Stop Lamp Wreath Emblem Assembly
2 | High Mounted Stop Lamp Crest Emblem Assembly Tip

• | Emblem is attached with double sided tape, use J 25070 heat gun or equivalent to aid in removal.

• | For additional information on emblem/nameplate replacement refer to Emblem/Nameplate Replacement.

#### Rear Compartment Lid Name Plate SLS Replacement

3 | Rear Compartment Lid Name Plate SLS Assembly

#### Procedure

1. For additional information on emblem/nameplate replacement refer to Emblem/Nameplate Replacement.
2. Dimension c is 63 mm (2.4 in) from the right vertical edge of the rear compartment lid.
3. Dimension d is 57 mm (2.2 in) from the level lower edge of the rear compartment lid.

#### Rear Compartment Lid Name Plate SGM

4 | Rear Compartment Lid Name Plate SGM

#### Procedure

1. For additional information on emblem/nameplate replacement refer to Emblem/Nameplate Replacement.
2. Dimension a is 4 mm (1.6 in) from the left vertical edge of the rear compartment lid.
3. Dimension b is 35 mm (1.38 in) from the level lower edge of the rear compartment lid.