For 1990-2009 cars

Callout | Component Name
--- | ---
Headlamp Bulb Replacement

• | Never open the high intensity discharge system ballast or the arc tube assembly starter.

• | Never probe between the high intensity discharge system ballast output connector and the arc tube assembly.

Preliminary Procedure

1. Remove the front fascia assembly. Refer to Fascia, Extension, Reinforcement and Impact Bar Replacement - Front Bumper in Bumpers.
2. Remove the Headlamp assembly. Refer to Headlamps, Fog Lamps, Turn Signal Lamps, Side Marker Lamps Replacement - Front.

1 | Headlamp Bulb Access Cover Screws (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 3 N·m (27 lb in)
2 | Headlamp Bulb Access Cover
3 | High Beam Headlamp Bulb Assembly Caution: Refer to Halogen Bulb Caution in the Preface section.
4 | Low Beam Headlamp Bulb Socket Assembly
5 | Low Beam Headlamp Bulb Assembly