For 1990-2009 cars

### Removal Procedure

1. Release the retaining clips using a blunt trim tool to remove center console panel. Refer to Front Floor Console Replacement.
2. Remove auxiliary HVAC control module retaining screws.
3. Remove auxiliary HVAC control module.
4. Disconnect auxiliary HVAC control module electrical connectors, remove the module.

### Installation Procedure

1. Connect the auxiliary HVAC control module electrical connectors.
2. Install auxiliary HVAC control module.

Caution: Refer to Fastener Caution in the Preface section.

3. Install auxiliary HVAC control module retaining screws.

Tighten
Tighten the screw to 2 N·m (80 lb in).

4. Install the center console panel. Refer to Front Floor Console Replacement.