For 1990-2009 cars

### Removal Procedure

1. Remove the defroster grille. Refer to Defroster Grille Replacement.
2. Remove the sunload sensor from the defroster grill by twisting the sensor ¼ turn counter clockwise.
3. Disconnect the sunload sensor electrical connector.
4. Remove the sunload sensor.

### Installation Procedure

1. Connect the sunload sensor electrical connector.
2. Install the sunload sensor to the defroster grille by twisting the sensor ¼ turn clockwise.
3. Install the defroster grille. Refer to Defroster Grille Replacement.