For 1990-2009 cars

### Removal Procedure

1. Remove the front floor console extension panel. Refer to Front Floor Console Extension Panel Replacement .
2. Remove the bolts securing the ashtray cigar lighter assembly trim panel.
3. Pry out the ashtray cigar lighter assembly trim panel, disconnect the electrical connector and remove the ashtray cigar lighter assembly.

### Installation Procedure

1. Connect the electrical connector and install the ashtray cigar lighter assembly trim panel.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts securing the ashtray cigar lighter assembly trim panel.

Tighten
Tighten the bolts to 9 N·m (80 lb in).

3. Install the front floor console extension panel. Refer to Front Floor Console Extension Panel Replacement .