For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the compressor assembly. Refer to Air Compressor Replacement.
3. Remove four screws from the air compressor shield.
4. Remove the shield.
5. Remove the hose (1) from the air dryer (2).
6. Remove the mounting screw (1).
7. Rotate the air dryer (1) to remove from compressor.

### Installation Procedure

1. Install the air dryer (1) to the compressor.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the air dryer mounting screw (1).

Tighten
Tighten the bolts to 6 N·m (53 lb in).

3. Install the hose (1) onto the air dryer (2).
4. Install the air compressor shield.

Tighten
Tighten the nut to 3 N·m(27 lb in).

5. Install the compressor to the vehicle. Refer to Air Compressor Replacement.
6. Lower the vehicle.