For 1990-2009 cars

### Removal Procedure

1. Remove the cooling fan assembly. Refer to Air Cleaner Inlet Duct Replacement.
2. Remove the fan blade retaining nut (1) from the motor.
3. Remove the fan blade from the motor shaft.
4. Remove the motor retaining screws (1).
5. Remove the motor from the shroud.

### Installation Procedure

1. Install the motor to the shroud.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the cooling fan motor retaining screws (1).

Tighten
Tighten the screws to 5 N·m (44 lb in).

3. Install the fan blade to the motor shaft.
4. Install the fan blade retaining nut (1) to the motor.

Tighten
Tighten the nut to 7 N·m (62 lb in).

5. Install the cooling fan assembly. Refer to Air Cleaner Inlet Duct Replacement.