For 1990-2009 cars

#### Special Tools

J 45059 Angle Meter

1. Install the oil pump drive spacer into the oil pump so that the drive flat engages the pump rotor.
2. Position the oil pump on the crankshaft.
3. Install the retaining bolts.

Caution: Refer to Fastener Caution in the Preface section.

4. Apply upward pressure on the pump while tightening the 3 retaining bolts. Tighten the bolts in the sequence (1-3) shown.

Tighten

1. First Pass--Tighten the oil pump mounting bolts in sequence to 10 N·m (89 lb in).
2. Final Pass--Tighten the oil pump mounting bolts in sequence an additional 35 degrees using the J 45059 .