For 1990-2009 cars

### Removal Procedure

1. Turn the ignition OFF.
2. Remove the front compartment sight shield, if necessary. Refer to Front Compartment Sight Shields Replacement .
3. Disconnect the camshaft position (CMP) sensor electrical connector.
4. Remove the CMP sensor bolt.
5. Remove the CMP sensor.

### Installation Procedure

1. Install the CMP sensor.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the CMP sensor bolt.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

3. Connect the CMP sensor electrical connector.
4. Install the front compartment sight shields as necessary. Refer to Front Compartment Sight Shields Replacement .