For 1990-2009 cars

## Oil Filter Adapter Installation Without Oil Cooler

1. Install a NEW gasket to the oil filter adapter.
2. Position the oil filter adapter on the crankcase.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the oil filter adapter bolts.

Tighten
Tighten the oil filter adapter bolts to 25 N·m (18 lb ft).

4. Fill the oil filter with oil.
5. Install the oil filter.

Tighten
Tighten the oil filter to 32 N·m (24 lb ft).

## Oil Filter Adapter Installation With Oil Cooler

1. Install a NEW gasket to the oil filter adapter.
2. Position the oil filter adapter on the crankcase.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the oil filter adapter bolts.

Tighten
Tighten the oil filter adapter bolts to 16 N·m (12 lb ft).

4. Fill the oil filter with oil.
5. Install the oil filter.

Tighten
Tighten the oil filter to 32 N·m (24 lb ft).