For 1990-2009 cars

Table 1: | 2-6 Clutch Plates Removal
Table 2: | 2-6 Clutch Piston Replacement
Table 3: | 2-6 Clutch Plates Installation

### 2-6 Clutch Plates Removal

Callout | Component Name
--- | ---
1 | 2-6 Clutch Backing Plate Retaining Ring
2 | 2-6 Clutch Backing Plate
3 | 2-6 Clutch Plate Assembly (Qty: 5)
4 | 2-6 Clutch Plate (Qty: 5)
5 | 2-6 Clutch (Waved) Plate

### 2-6 Clutch Piston Replacement

Callout | Component Name
--- | ---
1 | 2-6 Clutch Spring Retaining Ring Tip Ensure the DT-48065 is centered over the clutch spring.

#### Special Tools

DT-48065 Clutch Spring Compressor

2 | 2-6 Clutch Spring Notice: Ensure the spring tabs are facing down during installation and that the tabs fit between the teeth on the piston. Failure to do so may cause damage to the clutch assembly.
3 | 2-6 Clutch Piston Assembly Tip It may be necessary to apply air to the apply passage in order to unseat the piston.

### 2-6 Clutch Plates Installation

Callout | Component Name
--- | ---
1 | 2-6 Clutch (Waved) Plate
2 | 2-6 Clutch Plates (Qty: 5) Tip Alternate between steel and fiber clutch plates.
3 | 2-6 Clutch Plate Assembly (Qty: 5) Tip Alternate between steel and fiber clutch plates.
4 | 2-6 Clutch Backing Plate
5 | 2-6 Clutch Backing Plate Retaining Ring
6 | 2-6 Clutch Apply Passage Tip Apply air to verify proper installation of all 2-6 clutch components.