For 1990-2009 cars

1. Disconnect and remove the brake booster hose from the upper intake manifold.
2. Remove the intake manifold brace bolts (1 and 2).
3. Remove the intake manifold brace.
4. Remove the positive crankcase ventilation (PCV) tube assembly bracket bolts.
5. Disconnect and remove the PCV tube assembly from the upper intake manifold and right camshaft cover.
6. Disconnect the (EVAP) hose from the upper intake manifold and EVAP solenoid.
7. Remove the EVAP solenoid bolt.
8. Remove the EVAP solenoid.
9. Remove the intake manifold bolts.
10. Remove the intake manifold assembly.
11. Remove the lower intake manifold gasket.