For 1990-2009 cars

### Removal Procedure

1. Remove the blower and air inlet assembly. Refer to Air Inlet Assembly Replacement .
2. Disconnect the electrical connector from the recirculation actuator.
3. Remove the recirculation actuator screws (1).
4. Remove the recirculation actuator.

### Installation Procedure

1. Install the recirculation actuator.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the recirculation actuator screws (1).

Tighten
Tighten the screws to 1 N·m (9 lb in).

3. Connect the electrical connector to the recirculation actuator.
4. Install the blower and air inlet assembly. Refer to Air Inlet Assembly Replacement .