For 1990-2009 cars

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Closely inspect each tire for proper and even bead seating.
3. If any of the tire beads were not properly or evenly seated, reseat the tire bead, then go to step 4. Refer to Tire Dismounting and Mounting.
4. Wrap the circumference of each tire with tape (1) in the center tread area.

Wrapping the tread with tape allows for a smooth and accurate reading of radial runout to be obtained.

5. Position the dial indicator on the taped portion of the tire tread such that the dial indicator is perpendicular to the tire tread surface.
6. Slowly rotate the tire and wheel assembly one complete revolution to find the low spot.
7. Set the dial indicator to zero at the low spot.
8. Slowly rotate the tire and wheel assembly one more complete revolution and measure the total amount of radial runout.

Specification
Maximum tire and wheel assembly radial runout - measured on-vehicle: 1.52 mm (0.060 in)

9. Position the dial indicator on a smooth portion of the tire sidewall, as close to the tread as possible, such that the dial indicator is perpendicular to the tire sidewall surface.
10. Slowly rotate the tire and wheel assembly one complete revolution to find the low spot. Ignore any jumps or dips due to sidewall splices.
11. Set the dial indicator to zero at the low spot.
12. Slowly rotate the tire and wheel assembly one more complete revolution and measure the total amount of lateral runout. Ignore any jumps or dips due to sidewall splices and attain an average runout measurement.

Specification
Maximum tire and Wheel Assembly Radial Runout - on-vehicle Measured : 1.52 mm (0.060 in)

13. Repeat steps 4 to 12 until all the tires and wheel assemblies radial and lateral runout measurements have been taken.
14. Lower the vehicle.