For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Cover and Pad Replacement
2. Disconnect the electrical connector.

3. Remove the rear seat armrest fasteners from rear seat back frame.

4. Remove the rear seat central armrest.

### Installation Procedure

1. Install the rear seat central armrest onto rear seat back.

Notice: Refer to Fastener Notice in the Preface section.

2. Install rear seat armrest screws.

Tighten
Tighten the screws to 9 N·m(80 lb ft).

3. Connect electrical connectors.
4. Install the rear seat cushion. Refer to Rear Seat Cushion Cover and Pad Replacement.