For 1990-2009 cars

Callout | Component Name
--- | ---

#### Front Side Door Lock Assembly Replacement

#### Preliminary Procedures

1. Remove the front side door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the front side door water deflector. Refer to Water Deflector - Front Side Door.

1 | Front Side Door Lock Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 5 N·m (44 lb in)
2 | Front Side Door Lock Assembly
3 | Front Side Door Lock Screw (Qty: 2) Tighten 9 N·m (80 lb in)
4 | Front Side Door Lock Assembly Tip

1. Raise the window to the full up position.
2. The following items will need to be disconnected for removal and reconnected for installation:

• | Lock cylinder rod

• | Outside handle lock rod by opening the clip

• | Lock assembly electrical connector

3. Remove the lock assembly from the door with the inside handle cable assembly attached.