For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement or Front Side Door Trim Panel Replacement .
2. Remove the door control module (1) by releasing the fixing nuts.
3. Disconnect the electrical connectors from the control module.

### Installation Procedure

1. Connect the electrical connectors to the control module (1).

Notice: Refer to Fastener Notice in the Preface section.

2. Fix the door module bracket onto the clip and tighten the nut.

Tighten
Tighten the door control module bracket fixing nuts to 6 N·m (53 lb in).

3. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement or Front Side Door Trim Panel Replacement .