For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Interior Lights Schematics Connector End View Reference: Lighting Systems Connector End Views
1 | Did you perform the Diagnostic System Check - Vehicle? | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 | Test the rear compartment lamp controlled ground circuit for a short to ground. Refer to Circuit Testing and Wiring Repairs . Did you find and correct the condition? | Go to Step 5 | Go to Step 3
3 | Inspect for poor connections at the harness connector of the rear compartment lid release actuator. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs . Did you find and correct the condition? | Go to Step 5 | Go to Step 4
4 | Replace the rear compartment lid release actuator. Refer to Rear Compartment Lid Interior Release Latch Handle Replacement . Did you complete the replacement? | Go to Step 5 | --
5 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2