For 1990-2009 cars

### Removal Procedure

1. Remove the wiper motor mini 7.5 A and 30 A fuses. The wiper motor fuses are located in the underhood fuse block.
2. Remove the windshield wiper arm assembly. Refer to Windshield Wiper Arm Replacement.
3. Remove air inlet grille (1,3). Refer to Air Inlet Grille Panel Replacement.
4. Remove the wiper motor module mounting bolts (3,5).
5. Disconnect the wiper motor electrical connector (4).
6. Remove the wiper motor module (1) from the vehicle.

### Installation Procedure

1. Place the wiper motor module into the vehicle.
2. Connect the wiper motor electrical connector (4).
3. Align the wiper module locator hole (7) to the pin located inside rail of the drive side fender.
4. Align the locator hole (6) to the hole in the pillar flange.

Caution: Refer to Fastener Caution in the Preface section.

5. Install the outer bolt (5).

Tighten
Tighten the outer bolt to 10 N·m (80 lb in).

6. Install the center bolt (3).

Tighten
Tighten the center bolt to 10 N·m (89 lb in).

7. Install the air inlet grille (1,3). Refer to Air Inlet Grille Panel Replacement.
8. Install the windshield wiper arm assembly. Refer to Windshield Wiper Arm Replacement.
9. Install the wiper motor fuses to the underhood fuse block.