For 1990-2009 cars

1. Remove the right exhaust manifold heat shield bolts.
2. Remove the right exhaust manifold heat shield.
3. Remove the right exhaust manifold bolts and nuts from the right cylinder head.
4. Remove the right exhaust manifold.
5. Remove the right exhaust manifold gasket.
6. Remove the right exhaust manifold studs from the right cylinder head.
7. Remove the right engine mount upper nut.
8. Remove the right engine mount.
9. Remove the right engine mount bracket bolts.
10. Remove the right engine mount bracket.