For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Backup Lamp to the Rear Compartment Lid Nut | 6 N·m | 53 lb in
Cornering Lamp to the Front Fascia | 2 N·m | 18 lb in
Daytime Running Lamp (DRL) Resistor Fastener | 12 N·m | 106 lb in
Bumper Fascia to Fender Bolt | 9 N·m | 80 lb in
Fog Lamp to the Front Fascia Bolts | 2 N·m | 18 lb in
Headlamp Leveling Sensors to the Vehicle Bolts | 9 N·m | 80 lb in
Headlamp to Mounting Panel Bolts | 6 N·m | 53 lb in
High Mounted Stop Lamp to the Rear Compartment Lid Nut | 6 N·m | 53 lb in
Tail Lamp to the Body Nut | 6 N·m | 53 lb in