For 1990-2009 cars

#### Special Tools

J 45845 Caster and Camber Adjusting Tool

1. Install the J 45845 to the lower control arm and the frame.
2. Loosen the lower control arm to frame bolt.

Caution: Refer to Fastener Caution in the Preface section.

3. Adjust the camber angle by turning the turnbuckle on J 45845 the until the specifications have been met.

Tighten
Tighten the bolt to 135 N·m (96 lb ft).

4. Verify that the camber is still within specifications. Refer to Wheel Alignment Specifications.
5. Adjust the rear toe. Refer to Rear Toe Adjustment.