For 1990-2009 cars

#### Special Tools

• | EN 46106 Flywheel Holding Tool

• | J 24420-C Harmonic Balancer Puller

• | J 38416-2 Crankshaft Button

1. Install the EN 46106 through the starter mounting hole.
2. Remove the crankshaft balancer bolt.
3. Install the J 38416-2 in the nose of the crankshaft.
4. Install the J 24420-C in order to remove the crankshaft balancer.
5. Pull the crankshaft balancer off by tightening the center bolt on the J 24420-C until the crankshaft balancer pulls off of the crankshaft end.
6. Remove the J 24420-C from the crankshaft balancer.