For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
2. Remove rear seat adjuster switch. Refer to Power Seat Switch Replacement .
3. Loose the caliper and the J retainer.
4. Remove the rear seat cushion cover.
5. Remove the fixing screws securing the blower to the rear seat cushion frame, disconnect the electrical connector, remove rear seat cushion frame.
6. Separate the calipers between the blower and heater, remove the blower.
7. Remove the heater from rear seat cushion to separate rear seat cushion from the heater.

### Installation Procedure

1. Install the heater to the rear seat cushion.
2. Install the blower to the heater.
3. Install the fixing screws between the blower and the rear seat cushion frame, connect the electrical connector and install the rear seat cushion frame.
4. Install the rear seat cushion cover onto the rear set cushion.
5. Install the J retainer and reinstall calipers.
6. Install rear seat adjuster switch. Refer to Power Seat Switch Replacement .
7. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .