For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation .
3. Support the lower control arm with a suitable jack.
4. Remove the trailing arm to the knuckle mounting nut and bolt.
5. Remove the trailing link to rear subframe nut and bolt.
6. Remove the trailing arm from the vehicle.

### Installation Procedure

1. Install the trailing arm into the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Support the lower control arm with a suitable jack for alignment of the trailing link and the knuckle.
3. Install the trailing link to frame bolt and nut.
4. Install the trailing arm to knuckle mounting bolt and nut.

Tighten

• | Tighten the trailing arm to frame nut to 153 N·m(113 lb ft).

• | Tighten the trailing arm to knuckle retaining bolt to 172 N·m(127 lb ft).

5. Install the tire and wheel. Refer to Tire and Wheel Removal and Installation .
6. Lower the vehicle.