For 1990-2009 cars

#### Special Tools

J 24319-B Steering Linkage and Tie Rod Puller

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation.
3. Loosen the outer tie rod jam nut (1).
4. Remove the outer tie rod retaining nuts.
5. Using J 24319-B disconnect the outer tie rod from the steering knuckle.

Note: Note the number of turns during removal and make a mark for installation.

6. Remove the outer tie rod from the inner tie rod.

### Installation Procedure

Note: Use the same number of turns that was used during removal.

1. Install the outer tie rod end to the inner tie rod. Do not tighten the jam nut at this time.
2. Connect the outer tie rod to the steering knuckle.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the outer tie rod retaining nut.

Tighten
Tighten the nut to 82 N·m (60 lb ft).

4. Install the tire and wheel. Refer to Tire and Wheel Removal and Installation.
5. Lower the vehicle.
6. Adjust the front toe. Refer to Wheel Alignment - Steering Wheel Angle and/or Front Toe Adjustment.