For 1990-2009 cars

### Removal Procedure

1. Remove the left and right A-pillar trim panels. Refer to Windshield Pillar Garnish Molding Replacement .
2. Remove the defroster grille.
3. Disconnect the sunload and twilight sentinel sensor electrical connector and remove the grille.

### Installation Procedure

1. Connect the sunload and twilight sentinel sensor electrical connector.
2. Install the defroster grille.
3. Install the left and right A-pillar trim panels. Refer to Windshield Pillar Garnish Molding Replacement.