For 1990-2009 cars

### Circuit Description

The Traction Off indicator is controlled by the instrument cluster via serial data messages from the EBCM. When the RIM sees the traction control switch input grounded through the momentary traction control switch, it sends a serial data message to the EBCM that tells the EBCM that the traction control switch has been pressed. The EBCM then disables traction control and sends a serial data message to the instrument cluster to turn on the Traction Off indicator on the instrument panel. Each time the ignition is cycled from OFF to ON, the traction control system is enabled.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. Use the scan tool to check the normal state of the Traction Off indicator control.

2. Ensures that the instrument cluster can operate the Traction Off indicator.

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Antilock Brake System Schematics Connector End View Reference: Antilock Brake System Connector End Views or Master Electrical Component List .
1 | Did you perform the Diagnostic System Check - Vehicle? | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 |

1. Install a scan tool.
2. Turn ON the ignition, with the engine OFF.
3. With a scan tool, observe the TCS Warning Indicator/Message parameter in the DRP/ABS/TCS data list.

Does the scan tool display OFF?

Go to Step 3

Go to Step 4

3 |

1. Turn OFF the ignition.
2. Turn ON the ignition, with the engine OFF.
3. Observe the Traction Off indicator on the instrument panel cluster (IPC) during the bulb check.

Does the Traction Off indicator illuminate during the bulb check and then turn OFF?

Go to Testing for Intermittent Conditions and Poor Connections

Go to Step 5

4 | Inspect for poor connections at the harness connector of the electronic brake control module (EBCM). Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs . Did you find and correct the condition? | Go to Step 8 | Go to Step 6
5 | Inspect for poor connections at the harness connector of the IPC. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs . Did you find and correct the condition? | Go to Step 8 | Go to Step 7
6 | Replace the EBCM. Refer to Diagnostic System Check - Vehicle for replacement, setup, and programming. Did you complete the replacement? | Go to Step 8 | --
7 | Replace the IPC. Refer to Control Module References for replacement, setup, and programming. Did you complete the replacement? | Go to Step 8 | --
8 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2