For 1990-2009 cars

#### Special Tools

• | J 8092 Universal Driver Handle

• | J 44766 Seal Installer

• | J 45000 Seal Remover

### Removal Procedure

1. Remove the transmission torque converter. Refer to Torque Converter Replacement.
2. Remove and discard the torque converter seal bolts.
3. Remove the torque converter seal using J 45000 .

### Installation Procedure

1. Assemble J 8092 onto J 44766 .
2. Install the torque converter seal onto the tool before installing into the case to prevent damage to the seal.

Note: Align the torque converter seal with the bolt holes.

3. Install the torque converter seal into the torque converter housing.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the torque converter seal bolts.

Tighten
Tighten the NEW torque converter seal bolts to 3.6 N·m (32 lb in).

5. Install the transmission torque converter. Refer to Torque Converter Replacement.