For 1990-2009 cars

### Removal Procedure

1. Remove the ashtray. Refer to Cigarette Lighter Receptacle Replacement.
2. Remove the radio. Refer to Radio Replacement.
3. Remove the HVAC control module retaining screws.
4. Remove the HVAC control module.
5. Disconnect the HVAC control module electrical connectors.

### Installation Procedure

1. Connect the HVAC control module electrical connectors.
2. Install the HVAC control module.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the HVAC control module retaining screws.

Tighten
Tighten the screws to 2 N·m (18 lb in).

4. Install the radio. Refer to Radio Replacement.
5. Install the ashtray. Refer to Cigarette Lighter Receptacle Replacement.