For 1990-2009 cars

Checks | Causes
--- | ---
Lug bolts for the Torque Converter (1) | Inspect for loose torque converter (1) lug bolts.
Input Sun Gear Thrust Washer (55) | Inspect for wear or damage.
Turbine Shaft Thrust Bearing Assembly (57) | Inspect for wear or damage.
2-6 and 3-5-R Clutch Hub Thrust Bearing Assembly (65) | Inspect the bearing for wear or damage.
Output Carrier Assembly (68) |

• | Inspect the carrier assembly for damaged pinion gears, thrush washers, pins, and rollers.

• | Inspect for a worn or damaged center support roller bearing assembly (485).

• | Inspect for damaged thrust bearings (486, 488).

• | Inspect the carrier assembly for damaged output carrier rear sun gear thrust bearing (captured).

Output Carrier Thrust Bearing Assembly (69) | Inspect the bearing for wear or damage.
Output Shaft Thrust Bearing Assembly (71) | Inspect the bearing for wear or damage.
1-2-3-4 Clutch Hub Thrust Bearing Assembly (63) | Inspect the bearing for wear or damage.
Turbine Shaft Thrust Bearing Assembly (57) | Inspect the bearing for wear or damage.