For 1990-2009 cars

### Removal Procedure

1. Remove the battery from the vehicle. Refer to Battery Replacement.
2. Remove the bolts from the battery tray.
3. Remove the battery tray from the vehicle.

### Installation Procedure

1. Install the battery tray into the vehicle.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the battery tray bolts and tighten to 6 N·m (53 lb in).
3. Install the battery into the vehicle. Refer to Battery Replacement.