For 1990-2009 cars

Caution: DO NOT use any mechanical device such as pliers or screwdrivers to disengage the connector. In order to prevent damage to the connector or harness wiring, both of the latches on the connector must be depressed with finger pressure only. When the latches are depressed the connector must then be pulled straight back without pulling on the wires in order to disengage. Failure to follow this procedure can lead to connector or wiring harness damage and failure.