For 1990-2009 cars

#### Special Tools

• | EN 46326 Flywheel Holding Tool

• | J 41998-B Crankshaft Balancer Installer

• | J 45059 Angle Meter

1. Position the crankshaft balancer on the nose of the crankshaft.
2. Press the crankshaft balancer in place using the J 41998-B .
3. Clean the crankshaft balancer bolt threads.
4. Apply engine oil to the crankshaft balancer bolt threads.

Caution: Refer to Fastener Caution in the Preface section.

5. Install the crankshaft balancer bolt.

Tighten

1. First Pass--Tighten the crankshaft balancer bolt to 50 N·m (37 lb ft).
2. Final Pass--Tighten the crankshaft balancer bolt an additional 150 degrees using the J 45059 .

6. Remove the EN 46326 from the engine block.